Ex 1 Flashing Red LED

Using the Thonny Shell

**>>>from gpiozero import LED**

**>>>red\_led = LED(14)**

**>>>red\_led.off()**

**>>>red\_led.on()**

**>>>red\_led.blink(on\_time=.5, off\_time=.5,n=5)**

**NOW WIRE UP THE BLUE LED IN THE SAME MANNER AND CONNECT THE POSITIVE PIN TO PIN 12**

**>>>blue\_led = LED(12)**

**NOW TRY TO FLASH IT LIKE THE RED LED ABOVE**